*********************************
Date   : Sun Aug 20 23:00:39 2006
Error Number: (19047)
Message: Copy sector failure, result = 1, drive = 1, sectors from 32 to 8420 amount 8388
Version: 8.3.0.1331 (Nov 28 2005, Build=1331)
OS Version: DOS v7.10
Command line arguments:
Active Switches :
       FAT32 Conversion
       Sure
       Force Cloning
       Reboot
PathName            : \01DEMT~1.MP3
DumpFile            : 
DumpPos             : 0
FlagImplode         : 0
FlagExplode         : 0

Operation Details :
  Total size.........15773
  MB copied..........15763
  MB remaining.......10
  Percent complete...99%
  Speed..............1464 MB/min
  Time elapsed.......10:46   
  Time remaining.....0:00   

Program Call Stack
AbortLog
Generic_Abort
BrCopyFAT
BrSendCloneLocal
CopyFatPartition
ProcessFATPartition
CopyPartition
ProcessAllPartitions
CopyAllPartitions
CopyDiskToDisk
CopyMainline
AttemptOperation
sub_main
main

Call Stack
  0x00319625
  0x0007c94e
  0x0007bc29
  0x0007b4b1
  0x0007cebb
  0x0000d901
  0x00014731
  0x00014812
  0x00016625
  0x0008d0e7
  0x0008c7b1
  0x0008c5e8
  0x00088f36
  0x000023a5
  0x000024dd
  0x0000510f
  0x00004327
  0x00326978
End Call Stack


Start heap available: 529727488
Cur   heap available: 395116544
Total Memory:         535756800

Conventional Memory
Inital Conventional Memory Size = 460784
Current Conventional Memory Size = 223216
Allocated
   1024 DpmiDjgpp.cpp:56
  33504 ghost.cpp:1386
     64 DiskDriveAccessExInt13.cpp:128
     64 DiskDriveAccessExInt13.cpp:128
  32768 IdeDmaServerPci.cpp:127
    528 IdeDmaServerPci.cpp:127
    528 IdeDmaServerPci.cpp:127
    528 IdeDmaServerPci.cpp:127
Free
     80 DiskDriveAccessExInt13.cpp:91
    512 DiskDriveAccessInt13.cpp:176
  32768 BlockDeviceDosDrive.cpp:375

Fat details:
  SRC:
  FatType..........32
  first_sect.......11245563
  ClusterSize......16384
  clusters.........2092445
  root_next_avail..0
  data_next_avail..0
  dir_sector.......32732
  root_sector......32728
  data_sector......32728
  FAT_sector.......5207
  DST:
  FatType..........32
  first_sect.......11550798
  ClusterSize......32768
  clusters.........1073581
  root_next_avail..0
  data_next_avail..490740
  dir_sector.......16809
  root_sector......16808
  data_sector......16808
  FAT_sector.......3865

NTFS details:
----------------

NTFS Global Flags:
----------------
	 contiguousWrite=1 forceDiskClusterMapping=0 
	 inhibitCHKDSK=1 ignoreBadLog=0 ignoreCHKDSKBit=0
	 enable_cache=0 xfrbuflen=0 
	 last_attr_type = 0 
	 loadExact = 0 
----------------

Disk Error Details

IDE Controller error:
Uncorrectable data error
Error          0x40
Device/Head    0xe0
Cylinder High  0xb0
Cylinder Low   0x4f
Sector Number  0x40
Sector Count   0x00
LBA Sector     11554624

Disk Info :
  remote.............0
  drive..............0
  sectors_used.......78236424
  estimated_used.....32304326
  pemax..............2
  Version............0

 # Ord Boot Id Ext     First        Num       Last       Used NTFS
 0  0   80   b No         63   11245437   11245500    1754456 No
 1  1    0   b Yes   11245563   66990987   78236550   30549869 No

Disk Info :
  remote.............0
  drive..............1
  sectors_used.......80276805
  estimated_used.....0
  pemax..............2
  Version............0

 # Ord Boot Id Ext     First        Num       Last       Used NTFS
 0  0   80   b No         63   11550672   11550735    2590800 No
 1  1    0   b Yes   11550798   68726007   80276805   30978360 No

Fixed Drives

Drive 128 SAMSUNG SV0411N S01RJ10Y804467
Int 13h
Total Sectors            16434495
Bytes per Sector         512
MB                       8024
Cylinders                1023
Heads                    255
Sectors per Track        63
Successful IO Count      0

Extended Int 13h
Total Sectors            78242976
Bytes per Sector         512
MB                       38204
Successful IO Count      0

IDE using PIO
Total Sectors            78242976
Bytes per Sector         512
MB                       38204
Cylinders                16383
Heads                    16
Sectors per Track        63
Successful IO Count      0

IDE using UDMA (Active)
Total Sectors            78242976
Bytes per Sector         512
MB                       38204
Cylinders                16383
Heads                    16
Sectors per Track        63
Successful IO Count      524176

Drive 129 Maxtor 6E040L0 E1T940VE
Int 13h
Total Sectors            16434495
Bytes per Sector         512
MB                       8024
Cylinders                1023
Heads                    255
Sectors per Track        63
Successful IO Count      0

Extended Int 13h
Total Sectors            80291135
Bytes per Sector         512
MB                       39204
Successful IO Count      0

IDE using PIO
Total Sectors            80291135
Bytes per Sector         512
MB                       39204
Cylinders                16383
Heads                    16
Sectors per Track        63
Successful IO Count      0

IDE using UDMA (Active)
Total Sectors            80291135
Bytes per Sector         512
MB                       39204
Cylinders                16383
Heads                    16
Sectors per Track        63
Successful IO Count      528033
Error Count (bad media)  3
Error Count (other)      0
Last Error
IDE Controller error:
Uncorrectable data error
Error          0x40
Device/Head    0xe0
Cylinder High  0xb0
Cylinder Low   0x4f
Sector Number  0x40
Sector Count   0x00
LBA Sector     11554624


Floppy Drives

Remote Drives
AsyncIo : 0
Image Devices

Key[1]   1:1
Key[2]   C:
Path     C:
Desc     C: 1:1 [WINXPSP2]
Type     FAT
Disk     0
Offset   63

Key[1]   1:2
Key[2]   E:
Path     E:
Desc     E: 1:2 []
Type     FAT
Disk     0
Offset   11245563

Key[1]   2:1
Key[2]   D:
Path     D:
Desc     D: 2:1 [WINXPSP2]
Type     FAT
Disk     1
Offset   63

Key[1]   2:2
Key[2]   F:
Path     F:
Desc     F: 2:2 []
Type     FAT
Disk     1
Offset   11550798

Key[1]   A:
Path     A:
Desc     A:
Type     Floppy


*********************************
