;
; WIAPFU.INF  -- Windows Image Acquisition (WIA) Still Image Setup File
; Copyright (c) 2005-2008 PFU Limited
; Manufacturer: PFU Limited
; fi-5110Cdj
;    for Windows (x64)

[Version]
Signature="$CHICAGO$"
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%Provider%
DriverVer=01/05/2009,9.23.1
CatalogFile=fi5110C-x64.cat
;;INFINFO=FUJITSU_STI_TWAIN_INF

[SourceDisksNames]
0 = %SRCDISK1%, "fjwia-x64.cab", 0000-0000

[SourceDisksFiles]
fi5110u-x64.dll=0
FJTWAIN.URL=0
fi5110ex-x64.dll=0
fi5110ex0409-x64.dll=0
fi5110ex0411-x64.dll=0
fi5110ex0407-x64.dll=0
fi5110ex040C-x64.dll=0
fi5110ex0410-x64.dll=0
fi5110ex0804-x64.dll=0
fi5110ex0C0A-x64.dll=0

[ControlFlags]
ExcludeFromSelect=*

[DestinationDirs]
; By default, files will be copied to \windows\system.
DefaultDestDir=11 ; System directory
FI5110U.CopyFiles=11

[Manufacturer]
;;%Mfg%=Models
%Mfg%=Models,NTamd64

[Models.NTamd64]
%USB\FUJITSU_fi-5110CdjU______0.DeviceDesc% = FI5110U.Scanner,USB\VID_04C5&PID_1097

[FI5110U.Scanner]
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
DeviceSubType=0x1
; STI_GENCAP_SUBSET, STI_GENCAP_WIA, 0, 0, 0, 0: 
Capabilities=0x33
Events=FI5110U.Events
DeviceData=FI5110U.DeviceData 
AddReg=FI5110U.Scanner.AddReg
CopyFiles=FI5110U.CopyFiles
ICMProfiles="sRGB Color Space Profile.icm"

[FI5110U.Scanner.Services]
Include=sti.inf
Needs=STI.USBSection.Services

[FI5110U.DeviceData]
Server=local
UI Class ID={C8042878-CE53-4c62-AA47-3F521FB71AA7}
Polltimeout=0x3E8,1
TwainDS="FUJITSU fi-5110Cdj"
ISIS="fi5110c.PXN"

[FI5110U.Events]
StartButton		= %StartButton%,	{A6C5A715-8C6E-11d2-977A-0000F87A926F},Not Used
Send1			= %Send1%,			{F5D8E3a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send2			= %Send2%,			{F5D8E4a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send3			= %Send3%,			{F5D8E5a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send4			= %Send4%,			{F5D8E6a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send5			= %Send5%,			{F5D8E7a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send6			= %Send6%,			{F5D8E8a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send7			= %Send7%,			{F5D8E9a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send8			= %Send8%,			{F5D8Eaa0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send9			= %Send9%,			{F5D8Eba0-CCA4-11d2-B118-00A0C93EE7E0},Not Used

[FI5110U.Scanner.AddReg]
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,"usbscan.sys"
HKR,,HardwareConfig,1,4
HKR,,USDClass,,"{E017B4CB-D5FF-4b6d-9B3A-426F1BA96B9F}"
HKCR,CLSID\{E017B4CB-D5FF-4b6d-9B3A-426F1BA96B9F},,,"fi-5110C USB STI USD"
HKCR,CLSID\{E017B4CB-D5FF-4b6d-9B3A-426F1BA96B9F}\InProcServer32,,,%11%\fi5110u-x64.dll
HKCR,CLSID\{E017B4CB-D5FF-4b6d-9B3A-426F1BA96B9F}\InProcServer32,ThreadingModel,,"Both" ; Apartment
HKCR,CLSID\{BB78EB0F-B6EA-4184-B5D5-759C12AC791C},,,"ShellExt Class"
HKCR,CLSID\{BB78EB0F-B6EA-4184-B5D5-759C12AC791C}\InProcServer32,,,%11%\fi5110ex-x64.dll
HKCR,CLSID\{BB78EB0F-B6EA-4184-B5D5-759C12AC791C}\InProcServer32,ThreadingModel,,"Apartment"
HKCR,CLSID\{C8042878-CE53-4c62-AA47-3F521FB71AA7}\shellex\PropertySheetHandlers\{BB78EB0F-B6EA-4184-B5D5-759C12AC791C},,,"PfuExt extension"

[FI5110U.CopyFiles]
fi5110u-x64.dll    ;Ignore version check and always copy file
fi5110ex-x64.dll
fi5110ex0409-x64.dll
fi5110ex0411-x64.dll
fi5110ex0407-x64.dll
fi5110ex040C-x64.dll
fi5110ex0410-x64.dll
fi5110ex0804-x64.dll
fi5110ex0C0A-x64.dll
FJTWAIN.url

[Strings]
SRCDISK1="WIA Fujitsu fi-5110Cdj Disk 1"
Provider="FUJITSU"
;;Mfg="FUJITSU" ; "PFU Limited"
Mfg="FUJITSU"
TimeChanged="File Time Changed"
SizeChanged="File Size Changed"
;;USBScanner.SvcDesc="USB Scanner Driver" ; or "Scanner device"
USBScanner.SvcDesc="USB Scanner Driver"
USB\FUJITSU_fi-5110CdjU______0.DeviceDesc = "fi-5110Cdj"
StartButton="Start button pressed"
ScanButton="Scan button pressed"
INFINFO="FUJITSU_STI_TWAIN_INF"
INFINFO2="FUJITSU_WIA_TWAIN_INF"
Send1="Send to 1"
Send2="Send to 2"
Send3="Send to 3"
Send4="Send to 4"
Send5="Send to 5"
Send6="Send to 6"
Send7="Send to 7"
Send8="Send to 8"
Send9="Send to 9"
Platform="-x64"

