;
; fi60F.INF  -- Windows Image Acquisition (WIA) Still Image Setup File
; Copyright (c) 2004-2007 PFU Limited
; Manufacturer: PFU Limited
; fi-60F
;    for Windows (x64)

[Version]
Signature="$CHICAGO$"
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%Provider%
DriverVer=05/20/2008,9.22.101
CatalogFile=fi60F-x64.cat

[SourceDisksNames]
0 = %SRCDISK1%, "fjwia-x64.cab", 0000-0000

[SourceDisksFiles]
fi60Fu-x64.dll=0
ippi4cmt-x64.dll=0
60f_0000.nal=0
FJTWAIN.URL=0
fi60Fex-x64.dll=0
fi60Fex0409-x64.dll=0
fi60Fex0411-x64.dll=0
fi60Fex0407-x64.dll=0
fi60Fex040C-x64.dll=0
fi60Fex0410-x64.dll=0
fi60Fex0804-x64.dll=0
fi60Fex0C0A-x64.dll=0

[ControlFlags]
ExcludeFromSelect=*

[DestinationDirs]
; By default, files will be copied to \windows\system.
DefaultDestDir=11 ; System directory
FI60FU.CopyFiles=11

[Manufacturer]
%Mfg%=Models,NTamd64

[Models]

[Models.NT]

[Models.NTamd64]
%USB\FUJITSU_fi-60FU__________0.DeviceDesc% = FI60FU.Scanner,USB\VID_04C5&PID_10C7
%USB\FUJITSU_fi-60FU__________0.DeviceDesc% = FI60FU.Scanner,USB\VID_04B8&PID_0116

[FI60FU.Scanner]
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
DeviceSubType=0x1
; STI_GENCAP_SUBSET, STI_GENCAP_WIA, 0, 0, 0, 0: 
Capabilities=0x33
;Events=FI60FU.Events
DeviceData=FI60FU.DeviceData 
AddReg=FI60FU.Scanner.AddReg
CopyFiles=FI60FU.CopyFiles
ICMProfiles="sRGB Color Space Profile.icm"

[FI60F.Scanner.Services]
Include=sti.inf
Needs=STI.SCSISection.Services

[FI60FU.Scanner.Services]
Include=sti.inf
Needs=STI.USBSection.Services

[FI60FU.DeviceData]
Server=local
UI Class ID={ADEEC757-71CD-4f72-8949-28101F10FF69}
Polltimeout=0x3E8,1
TwainDS="FUJITSU fi-60F"
ISIS="fi60F.PXN"
MaxXferSize=512,1

;[FI60FU.Events]
;StartButton		= %StartButton%,	{A6C5A715-8C6E-11d2-977A-0000F87A926F},Not Used
;FeederLoaded	= %FeederLoaded%,	{F5D8E1a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
;Send1			= %Send1%,			{F5D8E3a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
;Send2			= %Send2%,			{F5D8E4a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
;Send3			= %Send3%,			{F5D8E5a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
;Send4			= %Send4%,			{F5D8E6a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
;Send5			= %Send5%,			{F5D8E7a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
;Send6			= %Send6%,			{F5D8E8a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
;Send7			= %Send7%,			{F5D8E9a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
;Send8			= %Send8%,			{F5D8Eaa0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
;Send9			= %Send9%,			{F5D8Eba0-CCA4-11d2-B118-00A0C93EE7E0},Not Used

[FI60FU.Scanner.AddReg]
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,"usbscan.sys"
HKR,,HardwareConfig,1,4
HKR,,USDClass,,"{A82B5D64-94EC-498a-A852-13496CB9D781}"
HKCR,CLSID\{A82B5D64-94EC-498a-A852-13496CB9D781},,,"fi-60F USB STI USD"
HKCR,CLSID\{A82B5D64-94EC-498a-A852-13496CB9D781}\InProcServer32,,,%11%\fi60Fu-x64.dll
HKCR,CLSID\{A82B5D64-94EC-498a-A852-13496CB9D781}\InProcServer32,ThreadingModel,,"Both" ; Apartment
HKCR,CLSID\{2D5FBE8D-3BD1-458c-BDD1-8A5F3848F110},,,"ShellExt Class"
HKCR,CLSID\{2D5FBE8D-3BD1-458c-BDD1-8A5F3848F110}\InProcServer32,,,%11%\fi60Fex-x64.dll
HKCR,CLSID\{2D5FBE8D-3BD1-458c-BDD1-8A5F3848F110}\InProcServer32,ThreadingModel,,"Apartment"
HKCR,CLSID\{ADEEC757-71CD-4f72-8949-28101F10FF69}\shellex\PropertySheetHandlers\{2D5FBE8D-3BD1-458c-BDD1-8A5F3848F110},,,"PfuExt extension"

[FI60FU.CopyFiles]
fi60Fu-x64.dll    ;Ignore version check and always copy file
ippi4cmt-x64.dll
60f_0000.nal
fi60Fex-x64.dll
fi60Fex0409-x64.dll
fi60Fex0411-x64.dll
fi60Fex0407-x64.dll
fi60Fex040C-x64.dll
fi60Fex0410-x64.dll
fi60Fex0804-x64.dll
fi60Fex0C0A-x64.dll
FJTWAIN.url

[Strings]
SRCDISK1="WIA Fujitsu fi-60F Disk 1"
Provider="FUJITSU"
;;Mfg="FUJITSU" ; "PFU Limited"
Mfg="FUJITSU"
TimeChanged="File Time Changed"
SizeChanged="File Size Changed"
USBScanner.SvcDesc="USB Scanner Driver"
USB\FUJITSU_fi-60FU__________0.DeviceDesc = "fi-60F"
;StartButton="Start button pressed"
;ScanButton="Scan button pressed"
;FeederLoaded="Feeder loaded with paper"
INFINFO="FUJITSU_STI_TWAIN_INF"
INFINFO2="FUJITSU_WIA_TWAIN_INF"
;Send1="Send to 1"
;Send2="Send to 2"
;Send3="Send to 3"
;Send4="Send to 4"
;Send5="Send to 5"
;Send6="Send to 6"
;Send7="Send to 7"
;Send8="Send to 8"
;Send9="Send to 9"
Platform="-x64"

