;
; WIAPFU.INF  -- Windows Image Acquisition (WIA) Still Image Setup File
; Copyright (c) 2005-2009 PFU Limited
; Manufacturer: PFU Limited
; fi-6800dj
;    for Windows (x64)

[Version]
;;Signature="$Windows NT$"
Signature="$CHICAGO$"
Class=Image
ClassGUID={6bdd1fc6-810f-11d0-bec7-08002be2092f}
Provider=%Provider%
DriverVer=01/08/2009,9.22.12
CatalogFile=fi6800-x64.cat
;;INFINFO=FUJITSU_STI_TWAIN_INF

[SourceDisksNames]
0 = %SRCDISK1%, "fi6800-x64.cab", 0000-0000

[SourceDisksFiles]
fi6800-x64.dll=0
fi6800u-x64.dll=0
FJTWAIN.URL=0
fi6800ex-x64.dll=0
fi6800ex0409-x64.dll=0
fi6800ex0411-x64.dll=0
;;fi6800ex0412-x64.dll=0
;;fi6800ex0407-x64.dll=0
;;fi6800ex040C-x64.dll=0
;;fi6800ex0410-x64.dll=0
;;fi6800ex0419-x64.dll=0
;;fi6800ex0804-x64.dll=0
;;fi6800ex0C0A-x64.dll=0
;;fi6800ex0404-x64.dll=0

[ControlFlags]
ExcludeFromSelect=*

[DestinationDirs]
; By default, files will be copied to \windows\system.
DefaultDestDir=11 ; System directory
FI6800.CopyFiles=11
FI6800U.CopyFiles=11

[Manufacturer]
;;%Mfg%=Models
%Mfg%=Models,NTamd64

[Models.NTamd64]
%SCSI\FUJITSU_fi-6800dj_______0.DeviceDesc% = FI6800.Scanner,FUJITSU_fi-6800dj_______0
%USB\FUJITSU__fi-6800U________0.DeviceDesc% = FI6800U.Scanner,USB\VID_04C5&PID_119D

[FI6800.Scanner]
Include=sti.inf
Needs=STI.SCSISection
SubClass=StillImage
DeviceType=1
DeviceSubType=0x1
; STI_GENCAP_SUBSET, STI_GENCAP_WIA, 0, 0, 0, 0: 
Capabilities=0x33
Events=Scan.Events
DeviceData=FI6800.DeviceData 
AddReg=FI6800.Scanner.AddReg
CopyFiles=FI6800.CopyFiles
ICMProfiles="sRGB Color Space Profile.icm"

[FI6800U.Scanner]
Include=sti.inf
Needs=STI.USBSection
SubClass=StillImage
DeviceType=1
DeviceSubType=0x1
; STI_GENCAP_SUBSET, STI_GENCAP_WIA, 0, 0, 0, 0: 
Capabilities=0x33
Events=Scan.Events
DeviceData=FI6800U.DeviceData 
AddReg=FI6800U.Scanner.AddReg
CopyFiles=FI6800U.CopyFiles
ICMProfiles="sRGB Color Space Profile.icm"

[FI6800.Scanner.Services]
Include=sti.inf
Needs=STI.SCSISection.Services

[FI6800U.Scanner.Services]
Include=sti.inf
Needs=STI.USBSection.Services

[FI6800.DeviceData]
Server=local
UI Class ID={A61297B7-57ED-4364-8E69-21CE2CB7C4B0}
Polltimeout=0x3E8,1
TwainDS="FUJITSU fi-6800dj"
ISISDriverName=fi6800.PXN

[FI6800U.DeviceData]
Server=local
UI Class ID={A61297B7-57ED-4364-8E69-21CE2CB7C4B0}
Polltimeout=0x3E8,1
TwainDS="FUJITSU fi-6800dj"
ISISDriverName=fi6800.PXN

[Scan.Events]
StartButton=%StartButton%,{A6C5A715-8C6E-11d2-977A-0000F87A926F},Not Used
Send1=%Send1%,{F5D8E3a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send2= %Send2%,{F5D8E4a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send3= %Send3%,{F5D8E5a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send4= %Send4%,{F5D8E6a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send5= %Send5%,{F5D8E7a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send6= %Send6%,{F5D8E8a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send7= %Send7%,{F5D8E9a0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send8= %Send8%,{F5D8Eaa0-CCA4-11d2-B118-00A0C93EE7E0},Not Used
Send9= %Send9%,{F5D8Eba0-CCA4-11d2-B118-00A0C93EE7E0},Not Used

Send10=%Send10%,{F5D8E2a0-CCA5-11d2-B118-00A0C93EE7E0},Not Used
Send11=%Send11%,{F5D8E3a0-CCA5-11d2-B118-00A0C93EE7E0},Not Used
Send12=%Send12%,{F5D8E4a0-CCA5-11d2-B118-00A0C93EE7E0},Not Used
Send13=%Send13%,{F5D8E5a0-CCA5-11d2-B118-00A0C93EE7E0},Not Used
Send14=%Send14%,{F5D8E6a0-CCA5-11d2-B118-00A0C93EE7E0},Not Used
Send15=%Send15%,{F5D8E7a0-CCA5-11d2-B118-00A0C93EE7E0},Not Used
Send16=%Send16%,{F5D8E8a0-CCA5-11d2-B118-00A0C93EE7E0},Not Used
Send17=%Send17%,{F5D8E9a0-CCA5-11d2-B118-00A0C93EE7E0},Not Used
Send18=%Send18%,{F5D8Eaa0-CCA5-11d2-B118-00A0C93EE7E0},Not Used
Send19=%Send19%,{F5D8Eba0-CCA5-11d2-B118-00A0C93EE7E0},Not Used

Send20=%Send20%,{F5D8E2a0-CCA6-11d2-B118-00A0C93EE7E0},Not Used
Send21=%Send21%,{F5D8E3a0-CCA6-11d2-B118-00A0C93EE7E0},Not Used
Send22=%Send22%,{F5D8E4a0-CCA6-11d2-B118-00A0C93EE7E0},Not Used
Send23=%Send23%,{F5D8E5a0-CCA6-11d2-B118-00A0C93EE7E0},Not Used
Send24=%Send24%,{F5D8E6a0-CCA6-11d2-B118-00A0C93EE7E0},Not Used
Send25=%Send25%,{F5D8E7a0-CCA6-11d2-B118-00A0C93EE7E0},Not Used
Send26=%Send26%,{F5D8E8a0-CCA6-11d2-B118-00A0C93EE7E0},Not Used
Send27=%Send27%,{F5D8E9a0-CCA6-11d2-B118-00A0C93EE7E0},Not Used
Send28=%Send28%,{F5D8Eaa0-CCA6-11d2-B118-00A0C93EE7E0},Not Used
Send29=%Send29%,{F5D8Eba0-CCA6-11d2-B118-00A0C93EE7E0},Not Used

Send30=%Send30%,{F5D8E2a0-CCA7-11d2-B118-00A0C93EE7E0},Not Used
Send31=%Send31%,{F5D8E3a0-CCA7-11d2-B118-00A0C93EE7E0},Not Used
Send32=%Send32%,{F5D8E4a0-CCA7-11d2-B118-00A0C93EE7E0},Not Used
Send33=%Send33%,{F5D8E5a0-CCA7-11d2-B118-00A0C93EE7E0},Not Used
Send34=%Send34%,{F5D8E6a0-CCA7-11d2-B118-00A0C93EE7E0},Not Used
Send35=%Send35%,{F5D8E7a0-CCA7-11d2-B118-00A0C93EE7E0},Not Used
Send36=%Send36%,{F5D8E8a0-CCA7-11d2-B118-00A0C93EE7E0},Not Used
Send37=%Send37%,{F5D8E9a0-CCA7-11d2-B118-00A0C93EE7E0},Not Used
Send38=%Send38%,{F5D8Eaa0-CCA7-11d2-B118-00A0C93EE7E0},Not Used
Send39=%Send39%,{F5D8Eba0-CCA7-11d2-B118-00A0C93EE7E0},Not Used

Send40=%Send40%,{F5D8E2a0-CCA8-11d2-B118-00A0C93EE7E0},Not Used
Send41=%Send41%,{F5D8E3a0-CCA8-11d2-B118-00A0C93EE7E0},Not Used
Send42=%Send42%,{F5D8E4a0-CCA8-11d2-B118-00A0C93EE7E0},Not Used
Send43=%Send43%,{F5D8E5a0-CCA8-11d2-B118-00A0C93EE7E0},Not Used
Send44=%Send44%,{F5D8E6a0-CCA8-11d2-B118-00A0C93EE7E0},Not Used
Send45=%Send45%,{F5D8E7a0-CCA8-11d2-B118-00A0C93EE7E0},Not Used
Send46=%Send46%,{F5D8E8a0-CCA8-11d2-B118-00A0C93EE7E0},Not Used
Send47=%Send47%,{F5D8E9a0-CCA8-11d2-B118-00A0C93EE7E0},Not Used
Send48=%Send48%,{F5D8Eaa0-CCA8-11d2-B118-00A0C93EE7E0},Not Used
Send49=%Send49%,{F5D8Eba0-CCA8-11d2-B118-00A0C93EE7E0},Not Used

Send50=%Send50%,{F5D8E2a0-CCA9-11d2-B118-00A0C93EE7E0},Not Used

[FI6800.Scanner.AddReg]
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,"scsiscan.sys"
HKR,,HardwareConfig,1,2
HKR,,USDClass,,"{9B43BB7C-ED39-4062-B039-8F6C168DB457}"
HKCR,CLSID\{9B43BB7C-ED39-4062-B039-8F6C168DB457},,,"fi-6800 STI USD"
HKCR,CLSID\{9B43BB7C-ED39-4062-B039-8F6C168DB457}\InProcServer32,,,%11%\fi6800-x64.dll
HKCR,CLSID\{9B43BB7C-ED39-4062-B039-8F6C168DB457}\InProcServer32,ThreadingModel,,"Both" ; Apartment
HKCR,CLSID\{023C42DA-2E66-4d3e-BEE0-688FBBE10522},,,"ShellExt Class"
HKCR,CLSID\{023C42DA-2E66-4d3e-BEE0-688FBBE10522}\InProcServer32,,,%11%\fi6800ex-x64.dll
HKCR,CLSID\{023C42DA-2E66-4d3e-BEE0-688FBBE10522}\InProcServer32,ThreadingModel,,"Apartment"
HKCR,CLSID\{A61297B7-57ED-4364-8E69-21CE2CB7C4B0}\shellex\PropertySheetHandlers\{023C42DA-2E66-4d3e-BEE0-688FBBE10522},,,"PfuExt extension"

[FI6800U.Scanner.AddReg]
HKR,,DevLoader,,*NTKERN
HKR,,NTMPDriver,,"usbscan.sys"
HKR,,HardwareConfig,1,4
HKR,,USDClass,,"{35F2F0DF-21D2-418f-873D-72256F8BA5EC}"
HKCR,CLSID\{35F2F0DF-21D2-418f-873D-72256F8BA5EC},,,"fi-6800 USB STI USD"
HKCR,CLSID\{35F2F0DF-21D2-418f-873D-72256F8BA5EC}\InProcServer32,,,%11%\fi6800u-x64.dll
HKCR,CLSID\{35F2F0DF-21D2-418f-873D-72256F8BA5EC}\InProcServer32,ThreadingModel,,"Both" ; Apartment
HKCR,CLSID\{023C42DA-2E66-4d3e-BEE0-688FBBE10522},,,"ShellExt Class"
HKCR,CLSID\{023C42DA-2E66-4d3e-BEE0-688FBBE10522}\InProcServer32,,,%11%\fi6800ex-x64.dll
HKCR,CLSID\{023C42DA-2E66-4d3e-BEE0-688FBBE10522}\InProcServer32,ThreadingModel,,"Apartment"
HKCR,CLSID\{A61297B7-57ED-4364-8E69-21CE2CB7C4B0}\shellex\PropertySheetHandlers\{023C42DA-2E66-4d3e-BEE0-688FBBE10522},,,"PfuExt extension"

[FI6800.CopyFiles]
fi6800-x64.dll     ;Ignore version check and always copy file
fi6800ex-x64.dll
fi6800ex0409-x64.dll
fi6800ex0411-x64.dll
;;fi6800ex0412-x64.dll
;;fi6800ex0407-x64.dll
;;fi6800ex040C-x64.dll
;;fi6800ex0410-x64.dll
;;fi6800ex0419-x64.dll
;;fi6800ex0804-x64.dll
;;fi6800ex0404-x64.dll
FJTWAIN.url

[FI6800U.CopyFiles]
fi6800u-x64.dll    ;Ignore version check and always copy file
fi6800ex-x64.dll
fi6800ex0409-x64.dll
fi6800ex0411-x64.dll
;;fi6800ex0412-x64.dll
;;fi6800ex0407-x64.dll
;;fi6800ex040C-x64.dll
;;fi6800ex0410-x64.dll
;;fi6800ex0419-x64.dll
;;fi6800ex0804-x64.dll
;;fi6800ex0404-x64.dll
FJTWAIN.url

[Strings]
SRCDISK1="WIA Fujitsu fi-6800dj Disk 1"
Provider="FUJITSU"
;;Mfg="FUJITSU" ; "PFU Limited"
Mfg="FUJITSU"
TimeChanged="File Time Changed"
SizeChanged="File Size Changed"
;;SCSIScanner.SvcDesc="SCSI Scanner Driver" ; or "Scanner device"
SCSIScanner.SvcDesc="SCSI Scanner Driver"
SCSI\FUJITSU_fi-6800dj_______0.DeviceDesc = "fi-6800dj"
;;USBScanner.SvcDesc="USB Scanner Driver" ; or "Scanner device"
USBScanner.SvcDesc="USB Scanner Driver"
USB\FUJITSU__fi-6800U________0.DeviceDesc = "fi-6800dj"
StartButton="Start button pressed"
ScanButton="Scan button pressed"
INFINFO="FUJITSU_STI_TWAIN_INF"
INFINFO2="FUJITSU_WIA_TWAIN_INF"
Send1="Send to 01"
Send2="Send to 02"
Send3="Send to 03"
Send4="Send to 04"
Send5="Send to 05"
Send6="Send to 06"
Send7="Send to 07"
Send8="Send to 08"
Send9="Send to 09"
Send10="Send to 10"
Send11="Send to 11"
Send12="Send to 12"
Send13="Send to 13"
Send14="Send to 14"
Send15="Send to 15"
Send16="Send to 16"
Send17="Send to 17"
Send18="Send to 18"
Send19="Send to 19"
Send20="Send to 20"
Send21="Send to 21"
Send22="Send to 22"
Send23="Send to 23"
Send24="Send to 24"
Send25="Send to 25"
Send26="Send to 26"
Send27="Send to 27"
Send28="Send to 28"
Send29="Send to 29"
Send30="Send to 30"
Send31="Send to 31"
Send32="Send to 32"
Send33="Send to 33"
Send34="Send to 34"
Send35="Send to 35"
Send36="Send to 36"
Send37="Send to 37"
Send38="Send to 38"
Send39="Send to 39"
Send40="Send to 40"
Send41="Send to 41"
Send42="Send to 42"
Send43="Send to 43"
Send44="Send to 44"
Send45="Send to 45"
Send46="Send to 46"
Send47="Send to 47"
Send48="Send to 48"
Send49="Send to 49"
Send50="Send to 50"
Platform="-x64"

